Logo

Description automatically generated

Equipment: **LVMCC-408A2** Location: **Utilities Building Main MCC**

**600 VAC**

**1000 mm**

**300 mm**

**0**

Shock Hazard when

**Covers are removed:**

Limited Approach**:**

Restricted Approach:

Glove Class:

**457 mm**

**2.7 cal/cm2**

**711 mm**

File: **NUT2113-2-RPT01** Date: **2022-MAY-19**

Arc Flash Analysis by:

**Arc Flash and Shock Hazard**

**SHOCK PROTECTION**

**ARC FLASH PROTECTION**

Std.: IEEE 1584-18

Working Distance:

Incident Energy:

Arc Flash Hazard Boundary:

Refer to CSA Z462 and the FNO energized work practice for PPE requirements